Graphics

Graphics

Pattern List

Ref.Code     Chem. Formula         Score    Scale Fac.  Mineral Name          
01-070-3755  Si O2                      67       0.905  Quartz                
00-024-0076  Fe S2                      50       0.041  Pyrite                
01-087-0691  ( K.94 Na.06 ) ( M..       42       0.169  Muscovite-2M1, mag..  
04-013-2805  Mg2.8 Fe1.75 Al2.7..       34       0.053  Clinochlore-1MIIb,..  
00-009-0466  Na Al Si3 O8               17       0.041  Albite, ordered       
00-001-0837  Ca C O3                     6       0.013  Calcite               
00-001-0942  Ca O · Mg O ·2 C O2         2       0.104  Dolomite              

Peak List

Pos.[°2Th.]  d-spacing [Å]  Rel. Int. [%]  Matched by
     6.2410       14.16234           1.71  04-013-2805       
     8.8471        9.99550          12.77  01-087-0691       
    12.5102        7.07573           7.34  04-013-2805       
    17.7467        4.99795           3.24  01-087-0691       
    18.8084        4.71813           1.23  04-013-2805       
    19.7937        4.48545           4.72  01-087-0691;04..  
    20.8543        4.25967          19.03  01-070-3755;04..  
    22.0489        4.03150           0.50  04-013-2805;00..  
    22.8844        3.88618           1.06  01-087-0691;04..  
    23.7873        3.74068           1.05  01-087-0691       
    24.2685        3.66759           0.81  00-009-0466       
    25.1705        3.53816           4.15  04-013-2805       
    25.4700        3.49433           1.63  01-087-0691;00..  
    26.6279        3.34773         100.00  01-070-3755;01..  
    27.9048        3.19737           3.04  01-087-0691;00..  
    28.5165        3.13016           1.75  00-024-0076;01..  
    29.3925        3.03632           0.38  00-001-0837       
    29.8417        2.99411           1.96  01-087-0691       
    30.7927        2.90377           0.50  00-001-0942       
    31.2214        2.86487           1.50  01-087-0691;00..  
    31.5919        2.82978           0.65  04-013-2805;00..  
    32.0523        2.79248           1.31  01-087-0691;00..  
    33.0278        2.71220           4.02  00-024-0076       
    34.5544        2.59579           2.18  01-087-0691;04..  
    34.9682        2.56602           4.46  01-087-0691;04..  
    35.9800        2.49408           0.53  01-087-0691;00..  
    36.5347        2.45951           6.52  01-070-3755;01..  
    37.0608        2.42580           2.57  00-024-0076;04..  
    37.5214        2.39509           1.26  01-087-0691;04..  
    37.8105        2.37941           1.06  01-087-0691;04..  
    39.4543        2.28398           5.84  01-070-3755;00..  
    40.0607        2.24893           0.61  01-087-0691;04..  
    40.2698        2.23959           3.13  01-070-3755;01..  
    40.7418        2.21473           1.82  00-024-0076;01..  
    41.9851        2.15019           0.71  01-087-0691;04..  
    42.4244        2.13070           5.07  01-070-3755;01..  
    45.3014        2.00185           2.40  01-087-0691;04..  
    45.7789        1.98208           3.01  01-070-3755;01..  
    47.3955        1.91817           1.95  00-024-0076;00..  
    50.1078        1.82052           8.84  01-070-3755;04..  
    54.8483        1.67386           2.79  01-070-3755;01..  
    55.3134        1.66088           1.87  01-070-3755;01..  
    55.7032        1.64881           1.09  01-087-0691;04..  
    56.2436        1.63560           3.19  00-024-0076;01..  
    59.0728        1.56384           0.27  00-024-0076;01..  
    59.9252        1.54362           5.82  01-070-3755;04..  
    61.7217        1.50293           2.04  00-024-0076;01..  
    63.9744        1.45534           1.03  01-070-3755;01..  
    65.9161        1.41710           0.26  01-070-3755;01..  
    67.7139        1.38264           2.97  01-070-3755;01..  
    67.9259        1.38227           1.88                    
    68.1312        1.37519           4.03  01-070-3755;01..  
    68.2226        1.37357           3.07  01-070-3755;01..  
    69.3868        1.35334           0.32  01-087-0691;04..  

Anchor Scan Parameters

Dataset Name:	MT 30
File name:	C:\XRD Data\MT 30.xrdml
Comment:	Configuration=Spinner Srage - Transmission, Owner=User-1, Creation date=11/5/2013 2:01:36 PM
	Goniometer=PW3050/60 (Theta/Theta); Minimum step size 2Theta:0.001; Minimum step size Omega:0.001
	Sample stage=Reflection-Transmission Spinner PW3064/60; Minimum step size Phi:0.1
	Diffractometer system=XPERT-PRO
	Measurement program=C:\Users\SEMCAL_XRD\Documents\Marcellus MSEEL\MT 30.xrdmp, Identifier={97745B73-CC68-4AD8-952B-424E8EDC9B8A}
	Batch program=C:\PANalytical\Data Collector\Programs\Xcelerator batch.xrdmp, Identifier={D91BE70E-4F93-42FA-94AC-AE5046DD9F66}
	MT 30
Measurement Date / Time:	6/15/2016 12:02:01 PM
Operator:	SEMCAL_XRD
Raw Data Origin:	XRD measurement (*.XRDML)
Scan Axis:	Gonio
Start Position [°2Th.]:	5.0084
End Position [°2Th.]:	69.9824
Step Size [°2Th.]:	0.0170
Scan Step Time [s]:	20.3200
Scan Type:	Continuous
PSD Mode:	Scanning
PSD Length [°2Th.]:	2.12
Offset [°2Th.]:	0.0000
Divergence Slit Type:	Fixed
Divergence Slit Size [°]:	0.2177
Specimen Length [mm]:	10.00
Measurement Temperature [°C]:	25.00
Anode Material:	Cu
K-Alpha1 [Å]:	1.54060
K-Alpha2 [Å]:	1.54443
K-Beta [Å]:	1.39225
K-A2 / K-A1 Ratio:	0.50000
Generator Settings:	40 mA, 45 kV
Diffractometer Type:	0000000011117966
Diffractometer Number:	0
Goniometer Radius [mm]:	240.00
Dist. Focus-Diverg. Slit [mm]:	100.00
Incident Beam Monochromator:	No
Spinning:	Yes

Document History

Insert Measurement:
- File name = "MT 30.xrdml"
- Modification time = "10/4/2017 2:34:37 PM"
- Modification editor = "SEMCAL_XRD"

Default properties:
- Measurement step axis = "None"
- Internal wavelengths used from anode material: Copper (Cu)
- Original K-Alpha1 wavelength = "1.54060"
- Used K-Alpha1 wavelength = "1.54060"
- Original K-Alpha2 wavelength = "1.54443"
- Used K-Alpha2 wavelength = "1.54443"
- Original K-Beta wavelength = "1.39225"
- Used K-Beta wavelength = "1.39225"
- Irradiated length = "10.00000"
- Receiving slit size = "0.10000"
- Step axis value = "0.00000"
- Offset = "0.00000"
- Sample length = "10.00000"
- Modification time = "10/4/2017 2:34:37 PM"
- Modification editor = "SEMCAL_XRD"

Interpolate Step Size:
- Derived = "Yes"
- Step Size = "0.01"
- Modification time = "10/4/2017 2:34:37 PM"
- Modification editor = "PANalytical"

Determine Background:
- Add to net scan = "Nothing"
- User defined intensity = "-5"
- Correction method = "Automatic"
- Bending factor = "2"
- Minimum significance = "1"
- Minimum tip width = "0.1"
- Maximum tip width = "1"
- Peak base width = "2"
- Use smoothed input data = "No"
- Granularity = "20"
- Modification time = "10/4/2017 1:21:36 PM"
- Modification editor = "SEMCAL_XRD"

Search Peaks:
- Minimum significance = "1"
- Minimum tip width = "0.1"
- Maximum tip width = "1"
- Peak base width = "2"
- Method = "Minimum 2nd derivative"
- Modification time = "4/28/2017 4:58:53 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "25.4700"
- Modification time = "10/4/2017 2:35:29 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "29.3925"
- Modification time = "10/4/2017 2:35:39 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "31.5919"
- Modification time = "10/4/2017 2:35:42 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "35.9800"
- Modification time = "10/4/2017 2:35:45 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "37.5214"
- Modification time = "10/4/2017 2:35:53 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "40.0607"
- Modification time = "10/4/2017 2:36:02 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "41.9851"
- Modification time = "10/4/2017 2:36:04 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "55.7032"
- Modification time = "10/4/2017 2:36:14 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "68.1312"
- Modification time = "10/4/2017 2:36:24 PM"
- Modification editor = "SEMCAL_XRD"

Search & Match:
- Allow pattern shift = "No"
- Auto residue = "Yes"
- Data source = "Profile and peak list"
- Demote unmatched strong = "Yes"
- Multi phase = "Yes"
- Restriction set = "Untitled"
- Restriction = "Restriction set"
- Subset name = ""
- Match intensity = "Yes"
- Two theta shift = "0"
- Identify = "No"
- Max. no. of accepted patterns = "5"
- Minimum score = "50"
- Min. new lines / total lines = "60"
- Search depth = "10"
- Minimum new lines = "5"
- Minimum scale factor = "0.1"
- Intensity threshold = "0"
- Use line clustering = "Yes"
- Line cluster range = "1.5"
- Search sensitivity = "1.8"
- Use adaptive smoothing = "Yes"
- Smoothing range = "1.5"
- Threshold factor = "3"
- Modification time = "10/4/2017 2:37:00 PM"
- Modification editor = "SEMCAL_XRD"

Delete Peak(s):
- Start position = "5.1936"
- End position = "5.1936"
- Modification time = "10/4/2017 2:38:25 PM"
- Modification editor = "SEMCAL_XRD"