Graphics

Graphics

Pattern List

Ref.Code     Chem. Formula         Score    Scale Fac.  Mineral Name          
01-070-3755  Si O2                      70       0.863  Quartz                
04-006-6835  Fe S2                      51       0.063  Pyrite, syn           
01-076-0927  ( Na0.84 Ca0.16 ) ..       19       0.036  Albite, calcian       
04-007-5003  K Al Si3 O8                17       0.225  Microcline            
00-005-0586  Ca C O3                    13       0.019  Calcite, syn          
01-075-1759  Ca Mg ( C O3 )2            21       0.021  Dolomite              
04-011-6849  K Al2 Si4 O10 ( O ..       30       0.209  Muscovite-2M1         

Peak List

Pos.[°2Th.]  d-spacing [Å]  Rel. Int. [%]  Matched by
     8.8491        9.99321           7.27  04-011-6849       
    17.7694        4.99160           2.01  04-011-6849       
    19.8022        4.48354           4.14  04-011-6849       
    20.8634        4.25782          19.28  01-070-3755;04..  
    22.0511        4.03111           0.74  01-076-0927;01..  
    22.9628        3.87308           0.51  01-076-0927;04..  
    23.5692        3.77479           0.86  01-076-0927;04..  
    23.8001        3.73559           0.67  04-011-6849       
    24.0253        3.70109           0.72  01-076-0927;01..  
    24.1520        3.68196           0.71  01-076-0927;04..  
    24.2931        3.66393           1.00  01-076-0927;04..  
    25.3967        3.50717           1.26  01-076-0927;04..  
    26.6368        3.34662         100.00  01-070-3755;04..  
    27.7487        3.21234           2.99  01-076-0927;04..  
    27.9421        3.19320           2.88  01-076-0927;04..  
    28.5397        3.12768           3.92  04-006-6835;04..  
    29.4293        3.03512           1.13  00-005-0586       
    29.8653        2.99180           1.13  01-076-0927;04..  
    30.9328        2.89094           1.79  01-075-1759       
    31.2572        2.85931           0.84  01-076-0927;04..  
    32.0054        2.79647           0.59  01-076-0927;04..  
    33.0360        2.71155           6.61  04-006-6835       
    34.5559        2.59353           1.45  04-007-5003;04..  
    34.7178        2.58181           1.70  04-007-5003;04..  
    34.9302        2.56872           3.10  04-007-5003;04..  
    36.5336        2.45958           5.84  01-070-3755;01..  
    37.0552        2.42615           3.98  04-006-6835;01..  
    37.3736        2.40422           0.71  01-076-0927;04..  
    37.7544        2.38281           1.06  01-076-0927;04..  
    39.4637        2.28345           5.65  01-070-3755;00..  
    40.2941        2.23830           2.50  01-070-3755;01..  
    40.7438        2.21462           2.83  04-006-6835;04..  
    42.4407        2.12992           4.76  01-070-3755;01..  
    45.3973        1.99784           1.37  01-076-0927;04..  
    45.7744        1.98226           2.98  01-070-3755;01..  
    47.4020        1.91793           2.50  04-006-6835;01..  
    50.1337        1.81964           9.84  01-070-3755;04..  
    52.0057        1.75846           0.34  01-076-0927;04..  
    54.8475        1.67388           2.47  01-070-3755;01..  
    55.3013        1.66122           1.33  01-070-3755;01..  
    55.7857        1.64657           0.54  01-076-0927;04..  
    56.2460        1.63554           5.13  04-006-6835;01..  
    58.7283        1.57089           0.37  01-076-0927;04..  
    58.9951        1.56572           0.64  04-006-6835;01..  
    59.9339        1.54342           5.20  01-070-3755;01..  
    61.6624        1.50424           1.78  04-006-6835;01..  
    61.8539        1.49880           1.28  01-076-0927;04..  
    63.9976        1.45367           0.96  01-070-3755;01..  
    64.2526        1.44971           1.71  04-006-6835;04..  
    67.7458        1.38321           3.29  01-070-3755;01..  
    68.1380        1.37506           4.31  01-070-3755;01..  
    68.3299        1.37281           3.97  01-070-3755;04..  

Anchor Scan Parameters

Dataset Name:	MT 11
File name:	C:\XRD Data\MT 11.xrdml
Comment:	Configuration=Spinner Srage - Transmission, Owner=User-1, Creation date=11/5/2013 2:01:36 PM
	Goniometer=PW3050/60 (Theta/Theta); Minimum step size 2Theta:0.001; Minimum step size Omega:0.001
	Sample stage=Reflection-Transmission Spinner PW3064/60; Minimum step size Phi:0.1
	Diffractometer system=XPERT-PRO
	Measurement program=C:\Users\SEMCAL_XRD\Documents\Marcellus MSEEL\MT 11.xrdmp, Identifier={1C401C9C-FA04-4752-A19E-23940A78C38D}
	Batch program=C:\PANalytical\Data Collector\Programs\Xcelerator batch.xrdmp, Identifier={15A30A00-6FD7-42F1-923A-CC77284190FA}
	MT 11
Measurement Date / Time:	6/14/2016 5:07:46 PM
Operator:	SEMCAL_XRD
Raw Data Origin:	XRD measurement (*.XRDML)
Scan Axis:	Gonio
Start Position [°2Th.]:	5.0084
End Position [°2Th.]:	69.9824
Step Size [°2Th.]:	0.0170
Scan Step Time [s]:	20.3200
Scan Type:	Continuous
PSD Mode:	Scanning
PSD Length [°2Th.]:	2.12
Offset [°2Th.]:	0.0000
Divergence Slit Type:	Fixed
Divergence Slit Size [°]:	0.2177
Specimen Length [mm]:	10.00
Measurement Temperature [°C]:	25.00
Anode Material:	Cu
K-Alpha1 [Å]:	1.54060
K-Alpha2 [Å]:	1.54443
K-Beta [Å]:	1.39225
K-A2 / K-A1 Ratio:	0.50000
Generator Settings:	40 mA, 45 kV
Diffractometer Type:	0000000011117966
Diffractometer Number:	0
Goniometer Radius [mm]:	240.00
Dist. Focus-Diverg. Slit [mm]:	100.00
Incident Beam Monochromator:	No
Spinning:	Yes

Document History

Insert Measurement:
- File name = "MT 11.xrdml"
- Modification time = "10/4/2017 1:16:58 PM"
- Modification editor = "SEMCAL_XRD"

Default properties:
- Measurement step axis = "None"
- Internal wavelengths used from anode material: Copper (Cu)
- Original K-Alpha1 wavelength = "1.54060"
- Used K-Alpha1 wavelength = "1.54060"
- Original K-Alpha2 wavelength = "1.54443"
- Used K-Alpha2 wavelength = "1.54443"
- Original K-Beta wavelength = "1.39225"
- Used K-Beta wavelength = "1.39225"
- Irradiated length = "10.00000"
- Receiving slit size = "0.10000"
- Step axis value = "0.00000"
- Offset = "0.00000"
- Sample length = "10.00000"
- Modification time = "10/4/2017 1:16:58 PM"
- Modification editor = "SEMCAL_XRD"

Interpolate Step Size:
- Derived = "Yes"
- Step Size = "0.01"
- Modification time = "10/4/2017 1:16:58 PM"
- Modification editor = "PANalytical"

Determine Background:
- Add to net scan = "Nothing"
- User defined intensity = "-5"
- Correction method = "Automatic"
- Bending factor = "2"
- Minimum significance = "1"
- Minimum tip width = "0.1"
- Maximum tip width = "1"
- Peak base width = "2"
- Use smoothed input data = "No"
- Granularity = "20"
- Modification time = "10/4/2017 1:21:36 PM"
- Modification editor = "SEMCAL_XRD"

Search Peaks:
- Minimum significance = "1"
- Minimum tip width = "0.1"
- Maximum tip width = "1"
- Peak base width = "2"
- Method = "Minimum 2nd derivative"
- Modification time = "4/28/2017 4:58:53 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "23.8001"
- Modification time = "10/4/2017 1:22:51 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "24.0253"
- Modification time = "10/4/2017 1:22:54 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "24.1520"
- Modification time = "10/4/2017 1:22:56 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "27.7487"
- Modification time = "10/4/2017 1:23:09 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "31.2572"
- Modification time = "10/4/2017 1:23:15 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "34.5559"
- Modification time = "10/4/2017 1:23:22 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "34.7178"
- Modification time = "10/4/2017 1:23:24 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "37.3736"
- Modification time = "10/4/2017 1:23:32 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "55.7857"
- Modification time = "10/4/2017 1:23:47 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "58.7283"
- Modification time = "10/4/2017 1:23:54 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "61.8539"
- Modification time = "10/4/2017 1:24:03 PM"
- Modification editor = "SEMCAL_XRD"

Insert Peak:
- Peak position [°2Th.] = "68.1380"
- Modification time = "10/4/2017 1:24:11 PM"
- Modification editor = "SEMCAL_XRD"

Search & Match:
- Allow pattern shift = "No"
- Auto residue = "Yes"
- Data source = "Profile and peak list"
- Demote unmatched strong = "Yes"
- Multi phase = "Yes"
- Restriction set = "Untitled"
- Restriction = "Restriction set"
- Subset name = ""
- Match intensity = "Yes"
- Two theta shift = "0"
- Identify = "No"
- Max. no. of accepted patterns = "5"
- Minimum score = "50"
- Min. new lines / total lines = "60"
- Search depth = "10"
- Minimum new lines = "5"
- Minimum scale factor = "0.1"
- Intensity threshold = "0"
- Use line clustering = "Yes"
- Line cluster range = "1.5"
- Search sensitivity = "1.8"
- Use adaptive smoothing = "Yes"
- Smoothing range = "1.5"
- Threshold factor = "3"
- Modification time = "10/4/2017 1:25:01 PM"
- Modification editor = "SEMCAL_XRD"